{"text_format":"3","workbook":"xls","n_sheets":7,"sheets":["招标汇总","工作室电脑","实训室电脑","实训机房布线","一体化布线","益智室多媒体","单购设备移机"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"招标汇总","index":0,"n_rows":9,"n_cols":6,"rows_kept":9,"merged":[[0,0,0,5],[8,0,8,1]],"flags":["formulas_cached_only"]}
["2020年暑期合肥科技职业学院实训机房及多媒体设备价格汇总"]
["序号","项目","数量","单位","金额","备注"]
[1,"工作室电脑",11,"台",0,"9台兼容机、2台品牌机"]
[2,"实训室电脑",61,"台",0,"61台计算机"]
[3,"实训机房布线（含桌椅）",1,"间",0,"多媒体设备及安装、北主楼实训室15张四人位操作台、61个方凳"]
[4,"一体化教室布线",1,"间",0,"含机位强弱电布线"]
[5,"益智工作室多媒体",1,"间",0,"多媒体设备及安装"]
[6,"单购设备移机",1,"批",0]
["招标总价",{"$nulls":3},0,"元"]

{"sheet":"工作室电脑","index":1,"n_rows":18,"n_cols":9,"rows_kept":18,"merged":[[0,0,0,8],[2,0,13,0],[14,0,16,0],[17,0,17,2],[17,6,17,7]],"flags":["formulas_cached_only"]}
["项目一：2020年暑期工作室计算机明细"]
["设备","序号","配置","规格参数","数量","单位","单价","合计","质保"]
["兼容机",1,"CPU","英特尔 酷睿i7-9700(原盒)",9,"块",null,0]
[null,2,"主板","华硕PRIME Z390-P",9,"块",null,0]
[null,3,"内存","海盗船16G-3200",9,"根",null,0]
[null,4,"显卡","华硕1660Ti-6G",9,"块",null,0]
[null,5,"机械硬盘","西部数据1TB 7200转",9,"块",null,0]
[null,6,"固态硬盘","三星981-256G M.2",9,"块",null,0]
[null,7,"显示器","冠捷 24B1XH",9,"台",null,0]
[null,8,"散热器","九州风神 玄冰400",9,"个",null,0]
[null,9,"电源","航嘉多核 WD500",9,"个",null,0]
[null,10,"机箱","先马 黑洞",9,"个",null,0]
[null,11,"键鼠","罗技 MK200 套件",9,"套",null,0]
[null,null,"小计","安装win10系统",9,"套",null,0,"元"]
["办公电脑\n（联想扬天T4900V）",1,"主机","主机（I5-9400 CPU，8GB内存，1TB机械硬盘，集成显卡，无光驱）",2,"台",null,0]
[null,2,"显示器","24英寸LED显示器",2,"台",null,0]
[null,null,"小计",null,2,"台",null,0,"元"]
["小 计",{"$nulls":5},0,null,"元"]

{"sheet":"实训室电脑","index":2,"n_rows":13,"n_cols":9,"rows_kept":13,"merged":[[0,0,0,8],[12,0,12,1]],"flags":["formulas_cached_only"]}
["项目二：2020年暑期实训机房计算机配置"]
["序号","配件","规格参数","数量","单位","单价","合计","质保","品牌"]
[1,"CPU","英特尔酷睿i5 9400F",61,"块",null,0]
[2,"主板","B365 主板",61,"块",null,0,null,"华硕、技嘉\n（中型板）"]
[3,"内存","16GB DDR4 3000",61,"根",null,0,null,"金士顿、海盗船"]
[4,"显卡","丽台P1000\n（或1660Ti-6G）",61,"块",null,0,null,"丽台、华硕、技嘉"]
[5,"机械硬盘","1TB 7200转 SATA3.0",61,"块",null,0,null,"西部数据、希捷"]
[6,"固态硬盘","三星981-256G M.2",61,"块",null,0]
[7,"电源","额定400W ",61,"个",null,0,null,"航嘉、鑫谷"]
[8,"显示器","21.5英寸IPS",61,"台",null,0,null,"冠捷、飞利浦"]
[9,"机箱","航嘉 GS400X",61,"个",null,0]
[10,"键盘鼠标","双飞燕KR-8572套装",61,"套",null,0]
["小 计",null,"安装win10系统",61,"套",null,0,"元"]

{"sheet":"实训机房布线","index":3,"n_rows":15,"n_cols":11,"rows_kept":15,"merged":[[0,0,0,10],[14,0,14,1],[14,6,14,7]],"flags":["formulas_cached_only"]}
["项目三：2020年暑期北主楼实训机房综合布线及多媒体安装"]
["序号","设备","品牌型号","规格参数","数量","单位","单价","合计","质保","品牌","备注"]
[1,"投影机",null,"流明：3800-4000\n分辨率：不低于1024*768\n对比度：不低于12000:1",1,"台",null,0,"整机质保不低于三年、灯泡不低于10000小时","品牌：索尼、日立、NEC "]
[2,"电动投影幕",null,"大小：120英寸\n比例：4:3",1,"张",null,0,null,"品牌：信鸽、红叶"]
[3,"吊架",null,"投影机专用吊架",1,"个",null,0]
[4,"钢制讲台\n（中控台）","圆杰YJ2200","一、外形尺寸(长*宽*高): 1200*700*900mm。\n二、结构：\n1、钢制结构；\n2、显示器钢罩背部须高出桌面40mm；\n3、可安装22英寸显示器，覆盖钢化玻璃；\n4、须和学校原有中控台钥匙保持统一。",1,"台",null,0]
[5,"中控","鹏畅P2000A","1、一键开关所有多媒体设备，\n2、一键切换，\n3、带本地电脑操作界面控制，\n5、联动控制投影机、投影幕。",1,"个",null,0]
[6,"功放",null,null,1,"台",null,0]
[7,"音箱",null,null,1,"对",null,0]
[8,"话筒",null,"一只领夹式、一只手持式",1,"对",null,0]
[9,"千兆交换机",null,"24口10/100/1000M自适应千兆非管理型交换机,背板带宽48Gbps,包转发率35.7Mbps，端口防雷4KV",3,"台",null,0,null,"华为、锐捷"]
[10,"61机位\n强弱电布线",null,"钢制机柜、国标VGA视频线、纯无氧铜国标音频线、一舟全铜芯六类双绞线、绿宝国标电源线、公牛多用插排、钢制阻燃线槽(地面)、PVC线槽(墙壁)",1,"批",null,0,null,null,"61机位强弱电布线"]
[11,"操作台","双人位操作台","材质：双饰面颗粒板，\n颜色：白色（与现有实训室一致），\n规格：长度：1500mm，宽度：600mm，高度：750mm，面板厚度：25mm，主机柜内径：不低于220mm，机柜内宽不低于450mm。",30,"张",null,0,null,null,"60机位电脑操作台，操作台两两固定、四人位联排摆放"]
[12,"方凳",null,"材质：多层板，\n颜色：与操作台一致，\n规格：面板长度：350mm，宽度：250mm，高度：450mm，面板厚度：25mm。",61,"个",null,0,null,null,"61张方凳（含教师一张）"]
["实训机房小计",null,null,"具体施工工艺投标前实地确认",1,"套",0,null,"元"]

{"sheet":"一体化布线","index":4,"n_rows":15,"n_cols":11,"rows_kept":15,"merged":[[0,0,0,10],[14,0,14,1],[14,6,14,7]],"flags":["formulas_cached_only"]}
["项目四：2020年暑期一体化教室综合布线及多媒体安装"]
["序号","设备","品牌型号","规格参数","数量","单位","单价","合计","质保","品牌","备注"]
[1,"计算机",null,"与实训机房电脑配置相同",1,"台",null,0]
[1,"投影机",null,"流明：3800-4000\n分辨率：不低于1024*768\n对比度：不低于12000:1",1,"台",null,0,"整机质保不低于三年、灯泡不低于10000小时","品牌：索尼、日立、NEC "]
[2,"电动投影幕",null,"大小：150英寸\n比例：4:3",1,"张",null,0,null,"品牌：信鸽、红叶"]
[3,"吊架",null,"投影机专用吊架",1,"个",null,0]
[4,"钢制讲台\n（中控台）","圆杰YJ2200","一、外形尺寸(长*宽*高): 1200*700*900mm。\n二、结构：\n1、钢制结构；\n2、显示器钢罩背部须高出桌面40mm；\n3、可安装22英寸显示器，覆盖钢化玻璃；\n4、须和学校原有中控台钥匙保持统一。",1,"台",null,0]
[5,"中控","鹏畅P2000A","1、一键开关所有多媒体设备，\n2、一键切换，\n3、带本地电脑操作界面控制，\n5、联动控制投影机、投影幕。",1,"个",null,0]
[6,"功放",null,null,1,"台",null,0]
[7,"音箱",null,null,1,"对",null,0]
[8,"话筒",null,"一只领夹式、一只手持式",1,"对",null,0]
[9,"千兆交换机",null,"24口10/100/1000M自适应千兆非管理型交换机,背板带宽48Gbps,包转发率35.7Mbps，端口防雷4KV",3,"台",null,0,null,"华为、锐捷"]
[10,"企业路由器",null,"5个千兆电口(4WAN/1LAN),1个USB端口，200兆带宽，100人以下中小企业",1,"台",null,0,null,"华为、锐捷"]
[11,"60个机位强弱电布线",null,"钢制机柜、国标VGA视频线、纯无氧铜国标音频线、一舟全铜芯六类双绞线、绿宝国标电源线、公牛多用插排、钢制阻燃线槽(地面)、PVC线槽(墙壁)。",1,"批",null,0,null,null,"60机位强弱电布线"]
["一体化小计",null,null,"具体施工工艺投标前实地确认",1,"套",0,null,"元"]

{"sheet":"益智室多媒体","index":5,"n_rows":13,"n_cols":11,"rows_kept":13,"merged":[[0,0,0,10],[12,0,12,1],[12,6,12,7]],"flags":["formulas_cached_only"]}
["项目五：2020年暑期益智工作室多媒体设备安装"]
["序号","设备","品牌型号","规格参数","数量","单位","单价","合计","质保","品牌","备注"]
[1,"电脑","联想扬天T4900V","I5-9400 CPU，8GB内存，1TB机械硬盘，21.5LED",1,"台",null,0,null,"联想"]
[2,"投影机",null,"流明：3800-4000\n分辨率：不低于1024*768\n对比度：不低于12000:1",1,"台",null,0,"整机质保不低于三年、灯泡不低于10000小时","品牌：索尼、日立、NEC "]
[3,"电动投影幕",null,"大小：120英寸\n比例：4:3",1,"张",null,0,null,"品牌：信鸽、红叶"]
[4,"吊架",null,"投影机专用吊架",1,"个",null,0]
[5,"钢制讲台\n（中控台）","圆杰YJ2200","一、外形尺寸(长*宽*高): 1200*700*900mm。\n二、结构：\n1、钢制结构；\n2、显示器钢罩背部须高出桌面40mm；\n3、可安装22英寸显示器，覆盖钢化玻璃；\n4、须和学校原有中控台钥匙保持统一。",1,"台",null,0]
[6,"中控","鹏畅P2000A",null,1,"个",null,0]
[7,"功放",null,null,1,"台",null,0]
[8,"音箱",null,null,1,"对",null,0]
[9,"话筒",null,"一只领夹式、一只手持式",1,"对",null,0]
[10,"布线",null,"国标VGA视频线、纯无氧铜国标音频线、一舟全铜芯超五类双绞线、绿宝国标电源线、公牛多用插排、钢制阻燃线槽(地面)、PVC线槽(墙壁)",1,"批",null,0]
["多媒体小计",null,null,"具体施工工艺投标前实地确认",1,"套",0,null,"元"]

{"sheet":"单购设备移机","index":6,"n_rows":10,"n_cols":11,"rows_kept":10,"merged":[[0,0,0,10],[6,2,6,3],[7,2,7,3],[8,2,8,3],[9,0,9,1],[9,2,9,3],[9,6,9,7]],"flags":["formulas_cached_only"]}
["项目六：2020年暑期单购设备及多媒体移机"]
["序号","设备","品牌型号","规格参数","数量","单位","单价","合计","品牌","质保","备注"]
[1,"投影机",null,"流明：3800-4000\n分辨率：不低于1024*768\n对比度：不低于12000:1",4,"台",0,0,"品牌：索尼、日立、NEC ","整机质保不低于三年、灯泡不低于10000小时","与实训机房投影机相同"]
[2,"投影幕",null,"大小：150英寸\n比例：4:3",4,"张",0,0,"品牌：信鸽、红叶"]
[3,"中控","鹏畅P2000A",null,3,"个",0,0]
[4,"显示器","冠捷 24B1XH",null,1,"台",0,0]
[5,"北主楼多媒体拆装及布线","    实训场地原有多媒体设备及线路拆装至另一间教室，并有30琴位简单布线，具体情况现场勘查。",null,1,"批",0,0,null,null,"北主五楼多媒体设备移至北主六楼"]
[6,"南主楼多媒体拆装","    实训场地原有多媒体设备及线路拆装至另一间教室，具体情况现场勘查。",null,1,"批",0,0,null,null,"南主二楼多媒体设备移至南主三楼"]
[7,"工作室布线","    工作室电脑布线",null,1,"批",0,0,null,null,"北主楼五楼工作室"]
["小 计",null,"具体施工工艺投标前实地确认",{"$nulls":3},0,null,"元"]